SwiftRMS
PERMIT TO WORK · CONFINED SPACE ENTRY
Confined Space Entry Permit Template
	Permit no.:  [  ]
	Site:  [  ]

	Confined space (location / ID):  [  ]
	Date:  [DD/MM/YYYY]

	Valid from (time):  [HH:MM]
	Valid until (time):  [HH:MM]

	Entry supervisor:  [  ]
	Top person / attendant:  [  ]

	RAMS / safe system of work ref.:  [  ]
	Linked permits (hot work, isolation):  [  ]


Part A. Why entry is needed
The Confined Spaces Regulations 1997 require you to avoid entry where it is reasonably practicable to do the work another way. Record the work and why it cannot be done from outside.
	


Part B. Hazards identified

☐  Lack of oxygen, or too much oxygen
☐  Toxic gas, fume or vapour
☐  Flammable or explosive atmosphere
☐  Flooding with liquid or free-flowing solids
☐  Excessive heat
☐  Dust
☐  Entrapment, moving parts or difficult access
Part C. Isolations

	Isolation (pipework, power, mechanical)
	Method (blank, valve locked, disconnected)
	Isolated by
	Proved by

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


Part D. Atmosphere testing
Test with a calibrated gas monitor before entry and at the intervals your safe system of work sets. Record the acceptable limits from your safe system of work in the first row.
	Time
	Oxygen %
	Flammable % LEL
	H2S ppm
	CO ppm
	Other
	Tested by

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


Part E. Controls and rescue

☐  Ventilation in place (natural or forced)
☐  Entrants trained and fit for the work
☐  Top person in place for the whole entry, with no other duties
☐  Communication method agreed and tested
☐  Rescue plan written and rescue team available
☐  Rescue equipment at the entrance (tripod and winch, harnesses, breathing apparatus as required)
☐  First aid and resuscitation equipment available
☐  How to call the emergency services, and the site address, known
	Rescue plan summary



Part F. Issue and acceptance

	Issued by (authorised person)

Name

Signature

Date
	Accepted by (entry supervisor)

Name

Signature

Date


Part G. Entry log

	No.
	Name
	Time in
	Time out
	Signature

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Part H. Hand-back and cancellation

☐  Everyone out and accounted for
☐  Tools and equipment removed
☐  Space closed and secured; isolations ready to remove
	Handed back by (entry supervisor)

Name

Signature

Date
	Permit cancelled by (issuer)

Name

Signature

Date


Read HSE's Approved Code of Practice L101, Safe work in confined spaces (hse.gov.uk/pubns/books/l101.htm), before planning entry. This blank template is not legal advice and does not replace a competent person's assessment.
swiftRMS · Generate a filled-in, task-specific RAMS in 2 minutes at swiftrms.co.uk/try
