SwiftRMS
PERMIT TO WORK · HOT WORK
Hot Work Permit Template
	Permit no.:  [  ]
	Site:  [  ]

	Exact location of work:  [  ]
	Date:  [DD/MM/YYYY]

	Valid from (time):  [HH:MM]
	Valid until (time, one shift at most):  [HH:MM]

	Contractor:  [  ]
	Person doing the hot work:  [  ]

	RAMS ref.:  [  ]
	Fire watch period after work:  [  ] minutes


Part A. The hot work
Tick the type of work and describe it. First ask whether a cold method (cutting, bolting, crimping) would do the job instead.
☐  Welding
☐  Cutting or burning
☐  Grinding
☐  Brazing or soldering
☐  Torch-on roofing
☐  Other (describe below)
	Description, and why a cold method is not practicable



Part B. Precautions before work starts

☐  Combustible materials removed from the area, or protected with fire-resistant covers
☐  Floor swept; gaps, openings and ducts covered so sparks cannot fall through
☐  Other side of walls, floors and ceilings checked for combustibles
☐  Suitable fire extinguishers at the work point, and the user trained
☐  Fire alarm arrangements agreed; any isolated detector heads recorded below
☐  Gas cylinders upright and secured, hoses checked, flashback arrestors fitted
☐  Ventilation or fume extraction in place
☐  Other trades and the site manager told; fire watcher appointed
	Detector heads isolated (location and who will reinstate them)



Part C. Issue and acceptance

	Issued by (authorised person)

Name

Signature

Date
	Accepted by (person doing the work)

Name

Signature

Date


Part D. Fire watch
The fire watcher stays during the work and for the period set above after it stops, then makes a final check of the area and the spaces around it.
	Fire watcher
	Hot work stopped
	Fire watch ended
	Final check by
	Time

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Part E. Completion and cancellation

☐  Area inspected after the fire watch: no smouldering or heat
☐  Detector heads reinstated
☐  Cylinders and equipment removed or stored safely
	Work completed by

Name

Signature

Date
	Permit cancelled by (issuer)

Name

Signature

Date


Check HSE's guidance on fire safety in construction (HSG168) and your insurer's hot work conditions, which may set specific distances and fire watch times. This blank template is not legal advice.
swiftRMS · Generate a filled-in, task-specific RAMS in 2 minutes at swiftrms.co.uk/try
