SwiftRMS
RISK ASSESSMENT & METHOD STATEMENT
Tilers RAMS Template
	Site / location:  [  ]
	Assessor (competent person):  [  ]

	Assessment date:  [DD/MM/YYYY]
	Review date:  [DD/MM/YYYY]

	Reference:  [  ]
	


Section 1 — Risk assessment

	No.
	Hazard
	Who might be harmed
	Existing control measures
	Likelihood (1-5)
	Severity (1-5)
	Risk (LxS)
	Additional controls required
	Residual L
	Residual S
	Residual risk
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	Common hazards for Tilers
Reference list to prompt your assessment — add each relevant hazard as a numbered row above.
Silica dust from cutting tiles and stone   ·   Dermatitis from adhesives and grout   ·   Knee injuries from prolonged kneeling   ·   Manual handling of heavy tiles and stone   ·   Cuts and lacerations from sharp edges   ·   Noise from wet and dry cutting equipment   ·   Slips on wet surfaces   ·   Electric shock from wet cutting equipment


Section 2 — Risk matrix key

	1-3  Low
	4-9  Medium-Low
	10-15  Medium-High
	16-25  High


Risk score = Likelihood (1-5) × Severity (1-5). Reassess after additional controls for the residual risk.
Section 3 — Method statement
Describe, step by step, how the work will be carried out safely.
	


Section 4 — Applicable legislation
Tick the regulations that apply to this work.
	☐  Health and Safety at Work etc. Act 1974 (HASAWA)
	☐  Management of Health and Safety at Work Regulations 1999 (MHSWR)

	☐  Construction (Design and Management) Regulations 2015 (CDM)
	☐  Work at Height Regulations 2005

	☐  Provision and Use of Work Equipment Regulations 1998 (PUWER)
	☐  Lifting Operations and Lifting Equipment Regulations 1998 (LOLER)

	☐  Control of Substances Hazardous to Health Regulations 2002 (COSHH)
	☐  Manual Handling Operations Regulations 1992

	☐  Control of Noise at Work Regulations
	☐  Electricity at Work Regulations


Section 5 — Sign-off

	Assessed by

Name

Signature

Date
	Reviewed / approved by

Name

Signature

Date


swiftRMS · Generate a filled-in, task-specific RAMS in 2 minutes at swiftrms.co.uk/try
